Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 37 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 39 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 41 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 51 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 52 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 53 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 55 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 56 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 57 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 65 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 72 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 106 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 112 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 152 : Using default destination of 1 (file).
Message[302] C:\EXAMPLES\16F876A\HS\HS\DEMO.ASM 152 : Register in operand not in bank 0.  Ensure that bank bits are correct.
