Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 29 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 30 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 71 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 72 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 77 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F876A\HS\HS\PWM2-AN.ASM 96 : Register in operand not in bank 0.  Ensure that bank bits are correct.
