Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 59 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 60 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 62 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] C:\EXAMPLES\16F877A\PICCOMM.ASM 78 : Using default destination of 1 (file).
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 114 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 115 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 116 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 118 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 119 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 120 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 129 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 136 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 168 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[302] C:\EXAMPLES\16F877A\PICCOMM.ASM 174 : Register in operand not in bank 0.  Ensure that bank bits are correct.
Message[305] C:\EXAMPLES\16F877A\PICCOMM.ASM 222 : Using default destination of 1 (file).
